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	41200
	Base out, erect, and dismantle tube and coupler scaffolding


	Kaupae | Level
	4

	Whiwhinga | Credit
	20

	Whāinga | Purpose
	This skill standard is for people intending to complete qualifications and credentials in the scaffolding trades.
People with this skill standard have the skills to plan and establish a safe area, erect tube and coupler scaffolding, check the structure for compliance, and dismantle tube and coupler scaffolding.
This skill standard aligns with the New Zealand Certificate in Scaffolding (Elementary) (Level 4) [Ref: 5659]. 


Hua o te ako me Paearu aromatawai | Learning outcomes and assessment criteria
	Hua o te ako | Learning outcomes 
	Paearu aromatawai | Assessment criteria

	1. Base out tube and coupler scaffolding.
	a. The components are positioned and erected in the correct sequence based on the required off-set distance and the width and length of each bay as required in accordance with the Good Practice Guidelines for Scaffolding in NZ.

	1. 
	b. Temporary bracing is attached, and the standards are levelled and aligned in accordance with the Good Practice Guidelines for Scaffolding in NZ.

	2. 
	c. Scaffold tags are used in accordance with the Good Practice Guidelines for Scaffolding in NZ.

	2. Build the working lift for tube and coupler scaffolding.
	a. The first working platform is erected from below (from ground level or a lower surface) including access in accordance with the Good Practice Guidelines for Scaffolding in NZ.

	3. 
	b. The platform is accessed and edge protection is installed using a safe method of work in accordance with the scaffold plan and the Good Practice Guidelines for Scaffolding in NZ.

	4. 
	c. The second working lift is erected using a safe method of work in accordance with the scaffold plan and the Good Practice Guidelines for Scaffolding in NZ.

	3.
Inspect the erected scaffold structure for compliance.
	a. The structure is checked for compliance with the scaffold plan in accordance with the Good Practice Guidelines for Scaffolding in NZ.

	5. 
	b. The inspection report is completed in accordance with the Good Practice Guidelines for Scaffolding in NZ and industry standards.

	6. 
	c. Changes are made where structure is not compliant to the Good Practice Guidelines for Scaffolding in NZ and the inspection report is amended accordingly.

	4.
Perform alterations and inspect the altered scaffold for compliance.
	a. Alteration involving the changing placement of a structural member is performed in accordance with the Good Practice Guidelines for Scaffolding in NZ and industry standards.

	7. 
	b. The altered scaffold is inspected and verified for compliance in accordance with the Good Practice Guidelines for Scaffolding in NZ and industry standards.

	5.   Dismantle tube and coupler scaffolding.
	a. The scaffold is dismantled in sequence in accordance with the Good Practice Guidelines for Scaffolding in NZ and worksite requirements.


Pārongo aromatawai me te taumata paearu | Assessment information and grade criteria
Assessment specifications:
The candidate must be capable of erecting and dismantling tube and coupler scaffolding.
This skill standard has been developed for learning and assessment on-job or off-job in a simulated environment. Where supervision is required by law, the supervisor must hold the appropriate Certificate of Competence for the scaffolding work undertaken.
Candidates may carry out practical scaffolding activities as part of a team. However, assessment must confirm that each candidate has independently demonstrated competence in all aspects of the required assessment criteria. Evidence must confirm that the candidate has actively and independently applied the relevant skills, knowledge, and safety behaviours across the full scope of the standard, including compliance with regulatory and site-specific requirements.
Competence requires a candidate to be capable of consistently performing the requirements:
· to current regulatory, industry and commercial standards 
· in commercial environments 
· with limited supervision
· in different and unfamiliar contexts. 
Definitions
Scaffolding is as defined in the latest versions of Good Practice Guidelines for Scaffolding in NZ and the Health and Safety in Employment Regulations 1995.
Scaffold plan refers to a key design document used as a basis for the erection of a particular scaffold. For this skill standard it must be prepared by the candidate.
Ngā momo whiwhinga | Grades available
Achieved
Ihirangi waitohu | Indicative content 
Technical skills and knowledge 
· Interpreting project instructions on agreed work to be carried out.
· Quality management systems.
· Regulatory, industry and Good Practice Guidelines for Scaffolding in NZ and manufacturer guidelines.
· Scaffold plans and the use of the correct sequence.
· Sequence in erecting and dismantling.
· Methods to maintain clean and tidy sites.
· Safe loading and unloading of tools, equipment, and product.
· Types of scaffold fittings, their purpose and limitations.
Communication, literacy and numeracy
· Relevant documentation.  
· Workplace communication.
· Interpersonal skills. 
· Measurement and calculations.
 
Rauemi | Resources 
Legislation available at http://legislation.govt.nz
· Health and Safety at Work Act 2015;
· The Good Practice Guidelines - Scaffolding in New Zealand (GPG), 2016 available from https://www.worksafe.govt.nz/topic-and-industry/working-at-height/scaffolding-in-new-zealand/;
and all subsequent amendments and replacements.
Pārongo Whakaū Kounga | Quality assurance information
	Ngā rōpū whakatau-paerewa | Standard Setting Body
	Construction and Specialist Trades Industry Skills Board

	Whakaritenga Rārangi Paetae Aromatawai | DASS classification
	Service Sector > Lifting Equipment > Elementary Scaffolding

	Ko te tohutoro ki ngā Whakaritenga i te Whakamanatanga me te Whakaōritenga | CMR
	0120


	Hātepe | Process
	Putanga | Version
	Rā whakaputa | Review Date
	Rā whakamutunga mō te aromatawai | Last date for assessment

	Rēhitatanga | Registration 
	1
	30 July 2026
	N/A

	Kōrero whakakapinga | Replacement information
	This skill standard replaced unit standards 20858, 23223 and 23224.

	Rā arotake | Planned review date
	31 December 2031


Please contact the Construction and Specialist Trades Industry Skills Board at info@cstisb.nz if you wish to suggest changes to the content of this skill standard.
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